Slide 10- recommended to use binary as the bridge

Slide 11- add 0s if the front isn’t in a full group

Slide 20- given four bits, what are the ranges?

sm/oc -2^(n - 1) -> 2^(n-1) -1

tc -2^(n-1) -> 2^(n-1)-1

ASCII questions possible, but not expected to memorize it